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Seismic Design Category – D (D1)
Live Load – 20 lbs
Ground Snow Load – 5 lb
Ultimate Wind Speeds 
Risk Category I = 105 (V-Ult)
Risk Category II = 115 (V-Ult)
Risk Category III = 120 (V-Ult)
Exposure C
Frost Depth – 24”

The following codes have been adopted by the City of Winnemucca (WMC 15.04):

2012 International Building Code 
2012 International Residential Code
2011 National Electrical Code
2012 Uniform Mechanical Code
2012 Uniform Plumbing Code
2012 International Fire Code
1997 Uniform Housing Code
2009 International Energy Conservation Code
1997 Uniform Code for the Abatement of Dangerous Buildings
2012 International Property Maintenance Code
2012 International Swimming Pool and Spa code
2009 ICC A117.1 Accessible and Usable Buildings and Facilities)


See Winnemucca Municipal Code 15.04 for amendments to the codes.



